<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<description>&lt;b&gt;Teledyne Relays&lt;/b&gt;&lt;p&gt;

Miniature Electromechanical Relays&lt;p&gt;
Hermetically Sealed, High Repeatability&lt;p&gt;
Failsafe and Magnetic-Latching styles&lt;p&gt;
High-Reliability, MIL-Spec, and Space Certified available</description>
<packages>
<package name="CG-TH-NOGND">
<description>Centigrid, Isolated from PCB</description>
</package>
<package name="TO5-10-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-8-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-6-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-8-SM">
<description>TO5, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="TO5-5-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-10-SM">
<description>TO5, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="TO5-7-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-8-SJ">
<description>TO5, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="TO5-8-J">
<description>TO5, Surface Mount J-lead</description>
</package>
<package name="TO5-10-SJ">
<description>TO5, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="TO5-10-J">
<description>TO5, Surface Mount J-lead</description>
</package>
<package name="121-TH-NOGND">
<description>RF121 (For Reference Only!) (Not Recommended for Application)</description>
</package>
<package name="TO5--TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="LB-TH-GND">
<description>Dual TO5, Fully Soldered</description>
</package>
<package name="LB-SM">
<description>Dual TO5, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="121-SM">
<description>GRF121</description>
</package>
<package name="121-TH-GND">
<description>RF121</description>
</package>
<package name="LB-TH-NOGND">
<description>Dual TO5, Isolated from PCB</description>
</package>
<package name="ECG-TH-NOGND">
<description>Extended Centigrid, Isolated from PCB</description>
</package>
<package name="ECG-SM">
<description>Extended Centigrid, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="CG-SM">
<description>Centigrid, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="TO5-7-SM">
<description>TO5, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="LB-SJ">
<description>Dual TO5, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="CG-SJ">
<description>Centigrid, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="ECG-SJ">
<description>Extended Centigrid, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="CG-J">
<description>Centigrid, Surface Mount J-lead</description>
</package>
<package name="TO5-5-SM">
<description>TO5, Surface Mount I-lead w/ Ground Shield</description>
</package>
<package name="255-TH-NOGND">
<description>1/2 Crystal Can, Isolated from PCB</description>
</package>
<package name="255-TH-GND">
<description>1/2 Crystal Can, Fully Soldered</description>
</package>
<package name="ECG-J">
<description>Extended Centigrid, Surface Mount J-lead</description>
</package>
<package name="ATTN-TH-NOGND">
<description>Extended Centigrid, Isolated from PCB</description>
</package>
<package name="ATTN-TH">
<description>Extended Centigrid, Fully Soldered</description>
</package>
<package name="CG-TH-GND">
<description>Centigrid, Fully Soldered</description>
</package>
<package name="ECG-TH-GND">
<description>Extended Centigrid, Fully Soldered</description>
</package>
<package name="TO5-6-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-8-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-10-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-7-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-7-J">
<description>TO5, Surface Mount J-lead</description>
</package>
<package name="TO5-7-SJ">
<description>TO5, Surface Mount J-lead w/ Ground Shield</description>
</package>
<package name="TO5-6A-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="TO5-6A-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-11-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-11-TH-GND">
<description>TO5, Fully Soldered</description>
</package>
<package name="CG-TH-Z">
<description>Centigrid, w/ Ground Pin "Z"</description>
</package>
<package name="CG-TH-Y">
<description>Centigrid, w/ Ground Pin "Y"</description>
</package>
<package name="ECG-TH-Z">
<description>Extended Centigrid, w/ Ground Pin "Z"</description>
</package>
<package name="ECG-TH-W">
<description>Extended Centigrid, w/ Ground Pin "W"</description>
</package>
<package name="ECG-TH-X">
<description>Extended Centigrid, w/ Ground Pin "X"</description>
</package>
<package name="ECG-TH-Y">
<description>Extended Centigrid, w/ Ground Pin "Y"</description>
</package>
<package name="TO5-5-TH-NOGND">
<description>TO5, Isolated from PCB</description>
</package>
<package name="TO5-5-TH-Y">
<description>TO5, w/ Ground Pin "Y"</description>
</package>
<package name="TO5-5-TH-Z">
<description>TO5, w/ Ground Pin "Z"</description>
</package>
<package name="ECG-116">
<description>Extended Centigrid</description>
</package>
<package name="ATTN-SM">
<description>Extended Centigrid, Surface Mount I-lead w/ Ground Shield</description>
</package>
</packages>
<symbols>
<symbol name="SPDT">
<pin name="COM" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="COIL">
<pin name="C-" direction="pas"/>
<pin name="C+" direction="pas"/>
</symbol>
<symbol name="NC-BYPASS">
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="DUAL-COIL">
<pin name="C-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="C2+" direction="pas"/>
</symbol>
<symbol name="LOOPBACK">
<pin name="C1" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="C2" direction="pas"/>
</symbol>
<symbol name="TTL-DUAL-COIL">
<pin name="+SUPPLY" direction="pas"/>
<pin name="G.A" direction="pas"/>
<pin name="G.B" direction="pas"/>
<pin name="-SUPPLY" direction="pas"/>
</symbol>
<symbol name="TTL-COIL">
<pin name="+SUPPLY" direction="pas"/>
<pin name="GATE" direction="pas"/>
<pin name="-SUPPLY" direction="pas"/>
</symbol>
<symbol name="NO-BYPASS">
<pin name="NC1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="NC2" direction="pas"/>
</symbol>
<symbol name="DPDT-T">
<pin name="COM" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="ATTN">
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="GND2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RF100_NO-GND">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$2" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="CG-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF300_NO-GND">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="TO5-8-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="COM" pad="8"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF310_NO-GND">
<description>RELAY

NC Bypass, Spring Return,

TO5, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="NC-BYPASS"/>
</gates>
<devices>
<device name="" package="TO5-6-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="NC1" pad="8"/>
<connect gate="G$2" pin="NC2" pad="2"/>
<connect gate="G$2" pin="NO1" pad="7"/>
<connect gate="G$2" pin="NO2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF300">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="TO5-8-SM">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="COM" pad="8"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="7"/>
<connect gate="G$4" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF342">
<description>RELAY

DPDT, Latching,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$5" symbol="GND"/>
</gates>
<devices>
<device name="" package="TO5-10-SM">
<connects>
<connect gate="G$1" pin="C+" pad="4"/>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$2" pin="C+" pad="9"/>
<connect gate="G$2" pin="C-" pad="10"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="G$5" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF341">
<description>RELAY

SPDT, Latching,

TO5, Hermetically Sealed

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$4" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="TO5-7-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="4"/>
<connect gate="G$1" pin="C-" pad="7"/>
<connect gate="G$2" pin="C+" pad="9"/>
<connect gate="G$2" pin="C-" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="6"/>
<connect gate="G$4" pin="NO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF700_NO-GND">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed,

Integrated Protection Diodes

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="TO5-8-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="COM" pad="8"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRF300">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="TO5-8-J">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="COM" pad="8"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF121">
<description>RELAY

SPDT, Latching,

50 Ohm Impedence matched, Hermetically Sealed

(Symbol shows Coil A last energized)</description>
<gates>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="DUAL-COIL"/>
<gate name="G$1" symbol="DPDT-T"/>
</gates>
<devices>
<device name="" package="121-TH-GND">
<connects>
<connect gate="G$1" pin="COM" pad="2"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="NO" pad="4"/>
<connect gate="G$2" pin="GND" pad="GND"/>
<connect gate="G$3" pin="C-" pad="5"/>
<connect gate="G$3" pin="C1+" pad="3"/>
<connect gate="G$3" pin="C2+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF121">
<description>RELAY

SPDT, Latching,

50 Ohm Impedence matched, Hermetically Sealed 

(Symbol shows Coil A last energized)</description>
<gates>
<gate name="G$1" symbol="DUAL-COIL"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="DPDT-T"/>
</gates>
<devices>
<device name="" package="121-SM">
<connects>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$2" pin="GND" pad="GND"/>
<connect gate="G$3" pin="COM" pad="2"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LB363">
<description>RELAY

Loopback, Spring Return,

Dual TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="LOOPBACK"/>
<gate name="G$2" symbol="LOOPBACK"/>
<gate name="G$3" symbol="COIL"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="LB-TH-GND">
<connects>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$2" pin="C1" pad="16"/>
<connect gate="G$2" pin="C2" pad="11"/>
<connect gate="G$2" pin="NC1" pad="14"/>
<connect gate="G$2" pin="NC2" pad="13"/>
<connect gate="G$3" pin="C+" pad="18"/>
<connect gate="G$3" pin="C-" pad="9"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GLB363">
<description>RELAY

Loopback, Spring Return,

Dual TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="LOOPBACK"/>
<gate name="G$2" symbol="LOOPBACK"/>
<gate name="G$3" symbol="COIL"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="LB-SM">
<connects>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$2" pin="C1" pad="16"/>
<connect gate="G$2" pin="C2" pad="11"/>
<connect gate="G$2" pin="NC1" pad="14"/>
<connect gate="G$2" pin="NC2" pad="13"/>
<connect gate="G$3" pin="C+" pad="18"/>
<connect gate="G$3" pin="C-" pad="9"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SGLB363">
<description>RELAY

Loopback, Spring Return,

Dual TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="GND"/>
<gate name="G$3" symbol="LOOPBACK"/>
<gate name="G$4" symbol="LOOPBACK"/>
</gates>
<devices>
<device name="" package="LB-SJ">
<connects>
<connect gate="G$1" pin="C+" pad="18"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="GND" pad="GND"/>
<connect gate="G$3" pin="C1" pad="2"/>
<connect gate="G$3" pin="C2" pad="7"/>
<connect gate="G$3" pin="NC1" pad="4"/>
<connect gate="G$3" pin="NC2" pad="5"/>
<connect gate="G$4" pin="C1" pad="16"/>
<connect gate="G$4" pin="C2" pad="11"/>
<connect gate="G$4" pin="NC1" pad="14"/>
<connect gate="G$4" pin="NC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SGRF300">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="SPDT"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="COIL"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="TO5-8-SJ">
<connects>
<connect gate="G$1" pin="COM" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NO" pad="3"/>
<connect gate="G$2" pin="COM" pad="8"/>
<connect gate="G$2" pin="NC" pad="6"/>
<connect gate="G$2" pin="NO" pad="7"/>
<connect gate="G$3" pin="C+" pad="1"/>
<connect gate="G$3" pin="C-" pad="9"/>
<connect gate="G$4" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF300">
<description>RELAY

DPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="TO5-8-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="COM" pad="8"/>
<connect gate="G$3" pin="NC" pad="6"/>
<connect gate="G$3" pin="NO" pad="7"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRF100">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="CG-J">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SGRF100">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="CG-SJ">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF100">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="CG-SM">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF100">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="CG-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF100-Y">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="CG-TH-Y">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF100-Z">
<description>RELAY

DPDT, Spring Return,

Centigrid, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="GND"/>
</gates>
<devices>
<device name="" package="CG-TH-Z">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="1"/>
<connect gate="G$2" pin="NC" pad="3"/>
<connect gate="G$2" pin="NO" pad="2"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="5"/>
<connect gate="G$3" pin="NO" pad="6"/>
<connect gate="G$4" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LB363_NO-GND">
<description>RELAY

Loopback, Spring Return,

Dual TO5, Hermetically Sealed

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="LOOPBACK"/>
<gate name="G$2" symbol="LOOPBACK"/>
<gate name="G$3" symbol="COIL"/>
</gates>
<devices>
<device name="" package="LB-TH-NOGND">
<connects>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$2" pin="C1" pad="16"/>
<connect gate="G$2" pin="C2" pad="11"/>
<connect gate="G$2" pin="NC1" pad="14"/>
<connect gate="G$2" pin="NC2" pad="13"/>
<connect gate="G$3" pin="C+" pad="18"/>
<connect gate="G$3" pin="C-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF180">
<description>RELAY

DPDT, Latching,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$5" symbol="GND"/>
</gates>
<devices>
<device name="" package="ECG-SM">
<connects>
<connect gate="G$1" pin="C+" pad="3"/>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$2" pin="C+" pad="8"/>
<connect gate="G$2" pin="C-" pad="10"/>
<connect gate="G$3" pin="COM" pad="2"/>
<connect gate="G$3" pin="NC" pad="4"/>
<connect gate="G$3" pin="NO" pad="1"/>
<connect gate="G$4" pin="COM" pad="7"/>
<connect gate="G$4" pin="NC" pad="6"/>
<connect gate="G$4" pin="NO" pad="9"/>
<connect gate="G$5" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF180">
<description>RELAY

DPDT, Latching,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$5" symbol="GND"/>
</gates>
<devices>
<device name="" package="ECG-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="3"/>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$2" pin="C+" pad="8"/>
<connect gate="G$2" pin="C-" pad="10"/>
<connect gate="G$3" pin="COM" pad="2"/>
<connect gate="G$3" pin="NC" pad="4"/>
<connect gate="G$3" pin="NO" pad="1"/>
<connect gate="G$4" pin="COM" pad="7"/>
<connect gate="G$4" pin="NC" pad="6"/>
<connect gate="G$4" pin="NO" pad="9"/>
<connect gate="G$5" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C_NO-GND">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-NOGND">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="116C">
<description>RELAY

DPDT, Failsafe, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$1" symbol="TTL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-116">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="1"/>
<connect gate="G$1" pin="-SUPPLY" pad="9"/>
<connect gate="G$1" pin="GATE" pad="10"/>
<connect gate="G$3" pin="COM" pad="2"/>
<connect gate="G$3" pin="NC" pad="4"/>
<connect gate="G$3" pin="NO" pad="3"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="6"/>
<connect gate="G$4" pin="NO" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
<gate name="GND" symbol="GND"/>
</gates>
<devices>
<device name="" package="ECG-TH-GND">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="GND" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C-W">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="GND" symbol="GND"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-W">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="GND" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C-X">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="GND" symbol="GND"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-X">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="GND" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C-Y">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="GND" symbol="GND"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-Y">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="GND" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="122C-Z">
<description>RELAY

DPDT, Latching, CMOS Interface,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="GND" symbol="GND"/>
<gate name="G$1" symbol="TTL-DUAL-COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-Z">
<connects>
<connect gate="G$1" pin="+SUPPLY" pad="10"/>
<connect gate="G$1" pin="-SUPPLY" pad="5"/>
<connect gate="G$1" pin="G.A" pad="4"/>
<connect gate="G$1" pin="G.B" pad="9"/>
<connect gate="G$3" pin="COM" pad="3"/>
<connect gate="G$3" pin="NC" pad="1"/>
<connect gate="G$3" pin="NO" pad="2"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="NC" pad="7"/>
<connect gate="G$4" pin="NO" pad="6"/>
<connect gate="GND" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF180_NO-GND">
<description>RELAY

DPDT, Latching,

Extended Centigrid, Hermetically Sealed

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
</gates>
<devices>
<device name="" package="ECG-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="3"/>
<connect gate="G$1" pin="C-" pad="5"/>
<connect gate="G$2" pin="C+" pad="8"/>
<connect gate="G$2" pin="C-" pad="10"/>
<connect gate="G$3" pin="COM" pad="2"/>
<connect gate="G$3" pin="NC" pad="4"/>
<connect gate="G$3" pin="NO" pad="1"/>
<connect gate="G$4" pin="COM" pad="7"/>
<connect gate="G$4" pin="NC" pad="6"/>
<connect gate="G$4" pin="NO" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF320_NO-GND">
<description>RELAY

NO Bypass, Spring Return,

TO5, Hermetically Sealed 

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="NO-BYPASS"/>
</gates>
<devices>
<device name="" package="TO5-6A-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="9"/>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="8"/>
<connect gate="G$2" pin="NC1" pad="4"/>
<connect gate="G$2" pin="NC2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF311">
<description>RELAY

SPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="GND"/>
<gate name="G$1" symbol="COIL"/>
</gates>
<devices>
<device name="" package="TO5-5-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="5"/>
<connect gate="G$2" pin="NC" pad="2"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF311_NO-GND">
<description>RELAY

SPDT, Spring Return,

TO5, Hermetically Sealed

(Recommended footprint for parts with spacer pad or placed with at least .025" clearance from PCB)</description>
<gates>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$1" symbol="COIL"/>
</gates>
<devices>
<device name="" package="TO5-5-TH-NOGND">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="5"/>
<connect gate="G$2" pin="NC" pad="2"/>
<connect gate="G$2" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GRF311">
<description>RELAY

SPDT, Spring Return,

TO5, Hermetically Sealed</description>
<gates>
<gate name="G$2" symbol="SPDT"/>
<gate name="G$3" symbol="GND"/>
<gate name="G$1" symbol="COIL"/>
</gates>
<devices>
<device name="" package="TO5-5-SM">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$2" pin="COM" pad="5"/>
<connect gate="G$2" pin="NC" pad="2"/>
<connect gate="G$2" pin="NO" pad="3"/>
<connect gate="G$3" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF255">
<description>RELAY

DPDT, Latching,

1/2 Crystal Can, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="255-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="8"/>
<connect gate="G$1" pin="C-" pad="10"/>
<connect gate="G$2" pin="C+" pad="3"/>
<connect gate="G$2" pin="C-" pad="5"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="9"/>
<connect gate="G$3" pin="NO" pad="1"/>
<connect gate="G$4" pin="COM" pad="2"/>
<connect gate="G$4" pin="NC" pad="4"/>
<connect gate="G$4" pin="NO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF257">
<description>RELAY

DPDT, Latching,

1/2 Crystal Can, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="COIL"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="SPDT"/>
<gate name="G$4" symbol="SPDT"/>
</gates>
<devices>
<device name="" package="255-TH-GND">
<connects>
<connect gate="G$1" pin="C+" pad="10"/>
<connect gate="G$1" pin="C-" pad="8"/>
<connect gate="G$2" pin="C+" pad="3"/>
<connect gate="G$2" pin="C-" pad="5"/>
<connect gate="G$3" pin="COM" pad="7"/>
<connect gate="G$3" pin="NC" pad="9"/>
<connect gate="G$3" pin="NO" pad="1"/>
<connect gate="G$4" pin="COM" pad="2"/>
<connect gate="G$4" pin="NC" pad="4"/>
<connect gate="G$4" pin="NO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A150">
<description>RELAY

Selectable Attenuator, Failsafe,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="ATTN"/>
<gate name="G$2" symbol="COIL"/>
</gates>
<devices>
<device name="" package="ATTN-TH">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1 GND"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$2" pin="C+" pad="3"/>
<connect gate="G$2" pin="C-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A152">
<description>RELAY

Selectable Attenuator, Failsafe,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="ATTN"/>
<gate name="G$2" symbol="COIL"/>
</gates>
<devices>
<device name="" package="ATTN-TH">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1 GND"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$2" pin="C+" pad="3"/>
<connect gate="G$2" pin="C-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GA152">
<description>RELAY

Selectable Attenuator, Failsafe,

Extended Centigrid, Hermetically Sealed</description>
<gates>
<gate name="G$1" symbol="ATTN"/>
<gate name="G$2" symbol="COIL"/>
<gate name="G$3" symbol="GND"/>
</gates>
<devices>
<device name="" package="ATTN-SM">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$2" pin="C+" pad="3"/>
<connect gate="G$2" pin="C-" pad="5"/>
<connect gate="G$3" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
